SeaRey Adventures
Progressive Aerodyne SeaRey Flight Training

Normal Water Takeoff Procedure
GIFFTS
Gear- Selected/Indicated/Verified up for water
Instruments-“in the green”
Flaps-30 degrees
Fuel Pumps-Both On
Trim-Full Aft
Situational Awareness-Winds/Boats/Waves/Terrain

-Begin Takeoff with stick full aft.  As aircraft comes on to step release back pressure or light forward stick.
-Hold takeoff pitch attitude until aircraft lifts off.
-Flaps 20 and climb at Vx-58 mph (if needed to clear obstacle). 
-Confirm gear up.
-Over any obstacles, flaps 10 and climb at Vy-63 mph.
-Reduce power below yellow arc on tachometer.
-Level off at 500’ agl, flaps up and reduce power to maintain 80 mph 
(approx. 4400 rpm) if staying in the pattern.





Normal Water Landing Procedure
GIFFTS (on downwind)
Gear- Selected/Indicated/Verified up for water
Instruments-“in the green”
Flaps-Up
Fuel Pumps-Both On
Trim-As required
Situational Awareness-Winds/Boats/Waves/Terrain/ Obstacles/Powerlines

-Abeam landing point, 3600-3800 RPM, Flaps 10, 75 mph, “Gear up for water”.
-On Base, Flaps 20, 70 mph, “Gear up for water”.
-On Final, Flaps 30, 65 mph, “Gear up for water”.
-Hold pitch attitude, reduce power slightly, touchdown at 48-52 mph.
-On touchdown, slight forward stick and reduce power to idle.
-Forward stick as aircraft slows, wings level.
-As aircraft comes off step full aft trim.

