SeaRey Adventures
Oral Prep Questions

Seaplane base markings on chart
Buoy colors and markings (Red right returning to shore)
Parts of the hull   Keel   Chine   Step    Bow   Stern
Ripples  2 kts
Crests break  10 kts
Whitecaps 15kts
Ways to determine wind direction on water.   Glassy area,  Streaks  (above 8 kts),  Waves perpendicular to wind.  Weathervaning for takeoff.  Smoke,Flags.  Groundspeed readout on GPS.
3 types of taxi    Idle/Plowing/Step
Porpoising  can occur if nose is  too high or too low.  Normally too low in Searey.
When do you abort? after 2 porpoises
Describe why it porpoises and how to stop it.
How do you approach a ramp with a crosswind?  Going downwind at an angle
VX  VY  VS  VSO  VNE Normal approach speed   Confined area speed
Glassy water technique
Empty Weight
Gross Weight
Considerations for solo flight?  Ballast and Direction of turn in water with wind? (only plow turn from upwind to downwind to get out of wind, plow turn from downwind to upwind can bury and break a float attach fitting)
Fuel system ops.  Number of fuel pumps?  Power source?  Failure modes?
Engine and turbo ops
TCU lights  Yellow/Red  what do they mean.  Red steady=overboost  Red Flashing=Takeoff power over 5 min. limit  Yellow=system failure or fault.
When to use TCU disengage switch?  Cautions?
“Choke” ops and description
Landing gear and tailwheel ops
Tailwheel not down. What to do?
Main gear stays up.  Options
Electric fire.  What to do?  Consequences?
Oil System.  How does it work?  Checking oil.
Engine cooling system.  Water loss consequences.  Certified 30 minutes with no water at full power
Ignition system description.   Separate windings on engine provide power in alternator section. CDI ignition. (capacitive discharge).











